Address = 0x000000ce  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:85:0:-1
Address = 0x000000ce  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:86:0:-1
Address = 0x000000d0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:87:0:-1
Address = 0x000000d2  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:88:0:-1
Address = 0x000000d4  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:83:0:-1
Address = 0x000000da  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:90:0:-1
Address = 0x000000dc  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:83:0:-1
Address = 0x000000e2  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:92:0:-1
Address = 0x000000e4  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:98:0:-1
Address = 0x000000e6  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:99:0:-1
Address = 0x000000e8  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:100:0:-1
Address = 0x000000ea  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:83:0:-1
Address = 0x000000f0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:102:0:-1
Address = 0x000000f2  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:83:0:-1
Address = 0x000000f8  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:104:0:-1
Address = 0x000000fa  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:107:0:-1
Address = 0x000000fe  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:108:0:-1
Address = 0x00000100  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:109:0:-1
Address = 0x00000102  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:110:0:-1
Address = 0x00000104  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:111:0:-1
Address = 0x00000106  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:105:0:-1
Address = 0x0000010e  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:113:0:-1
Address = 0x00000114  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:105:0:-1
Address = 0x0000011e  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:115:0:-1
Address = 0x00000124  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:105:0:-1
Address = 0x0000012a  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:117:0:-1
Address = 0x00000130  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:105:0:-1
Address = 0x00000138  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:119:0:-1
Address = 0x0000013e  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:120:0:-1
Address = 0x00000144  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:121:0:-1
Address = 0x0000014a  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:122:0:-1
Address = 0x00000150  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:123:0:-1
Address = 0x00000156  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:105:0:-1
Address = 0x0000015c  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:125:0:-1
Address = 0x00000162  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:133:0:-1
Address = 0x00000166  File:line:col:begin = c:/winavr-20100110/lib/gcc/../../avr/include/util/delay_basic.h:83:0:-1
Address = 0x0000016c  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:135:0:-1
Address = 0x0000016e  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:136:0:-1
Address = 0x00000172  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:137:0:-1
Address = 0x00000174  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:138:0:-1
Address = 0x00000178  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:139:0:-1
Address = 0x0000017c  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:141:0:-1
Address = 0x00000186  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:141:0:-1
Address = 0x000001a0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:143:0:-1
Address = 0x000001c6  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:144:0:-1
Address = 0x000001d0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:143:0:-1
Address = 0x000001d6  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:146:0:-1
Address = 0x000001fa  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:147:0:-1
Address = 0x00000206  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:149:0:-1
Address = 0x00000208  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:148:0:-1
Address = 0x0000020c  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:149:0:-1
Address = 0x00000220  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:148:0:-1
Address = 0x00000226  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:151:0:-1
Address = 0x00000238  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:154:0:-1
Address = 0x00000244  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:156:0:-1
Address = 0x00000246  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:159:0:-1
Address = 0x00000254  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:162:0:-1
Address = 0x0000025e  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:163:0:-1
Address = 0x00000262  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:161:0:-1
Address = 0x00000268  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:167:0:-1
Address = 0x00000276  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:170:0:-1
Address = 0x00000280  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:171:0:-1
Address = 0x00000284  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:169:0:-1
Address = 0x0000028a  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:175:0:-1
Address = 0x00000296  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:178:0:-1
Address = 0x000002a0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:179:0:-1
Address = 0x000002a4  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:177:0:-1
Address = 0x000002b0  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:186:0:-1
Address = 0x000002ba  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:187:0:-1
Address = 0x000002be  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:185:0:-1
Address = 0x000002c4  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:192:0:-1
Address = 0x000002d2  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:193:0:-1
Address = 0x000002da  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:196:0:-1
Address = 0x000002de  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:200:0:-1
Address = 0x000002e2  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:202:0:-1
Address = 0x000002e6  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:203:0:-1
Address = 0x000002ea  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:207:0:-1
Address = 0x000002ee  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:208:0:-1
Address = 0x000002f2  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:209:0:-1
Address = 0x000002f6  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:213:0:-1
Address = 0x000002fa  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:212:0:-1
Address = 0x00000300  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:213:0:-1
Address = 0x00000308  File:line:col:begin = C:\Winavr+AvrStudio\AVR-A2\ADC_CDS_Thermi\default/../TEST_Source.c:213:0:-1
